#
TRANSMITTER BATTERY REPLACEMENT

BME0914675DY201

## Normal Key Type

1. Insert a small flathead screwdriver into the slot and gently pry open the transmitter.

2. Remove the battery.

3. Install the new batteries with the positive pole (+) facing down.

Battery specification

  Lithium CR2025 × 1

  Note

  • The batteries will last about 2 years when used 10 times a day.

4. Align the front and back covers. (1)

5. Snap the transmitter shut. (2)

## Retractable Key Type

1. Insert a small screwdriver into the slot and push the tab to remove the key from the transmitter.

2. Insert a small screwdriver into the slot and gently pry open the transmitter.

3. Remove the battery.

4. Put in the new battery (CR1620) with the positive pole (+) facing down.

5. Align the front and back covers and snap the transmitter shut.

Battery specification

  Lithium CR1620 × 1

  Note

  • The batteries will last about 2 years when used 10 times a day.

6. Install the key to the transmitter.