#
CRUISE CONTROL MODULE FUNCTION

BME012066320T01

## Tap up/Tap down Function

• When the vehicle is driving at a constant speed set by the cruise control system, and a signal from either the SET/COAST or RESUME/ACCEL switch is sent to the cruise control module for a very short period (a one-touch control function), the cruise control module increases or decreases the vehicle speed by 1 MPH {1.6 km/h}.