#
LATCH RELEASE ACTUATOR REMOVAL/INSTALLATION

BME091172380201

1. Close the rear door glass completely.

2. Disconnect the negative battery cable.

3. Remove the sliding door trim.

4. Remove the door screen.

5. Disconnect the sliding door lock actuator connector.

6. Disconnect the rods and the cables.

7. Remove the bolts, and remove the sliding door remote controller.

8. Disconnect the latch release actuator connector.

9. Remove the screws, and remove the latch release actuator from the sliding door remote controller.

10. Install in the reverse order of removal.