#
HOLD SWITCH INSPECTION [FN4A-EL]

BME051719200201

## Inspection of Operation

1. Turn the ignition switch from the LOCK to the ON position.

2. Verify that the HOLD indicator light is not illuminated. Press the HOLD switch and verify that the HOLD indicator light illuminates.

  • If not as specified, inspect the terminal voltage of the HOLD switch.

## Inspection of Voltage

1. Turn the ignition switch to the ON position.

2. Measure the voltage at the HOLD switch connector.

  • If not as specified, inspect the HOLD switch for continuity. (See Inspection of Continuity.)

Position | Terminal
--- | ---
I | J
OFF (Normal) | (V) | 0 | B+
ON (Depressed) | (V) | 0 | 0

  (V) :
Voltage

## Inspection of Continuity

1. Disconnect the HOLD switch connector.

2. Inspect the HOLD switch for continuity.

  • If the switch is normal, inspect the wiring harness. (HOLD switch-PCM, HOLD switch-Body ground.)
  • If not as specified, replace the selector lever component. (See SELECTOR LEVER REMOVAL/INSTALLATION.)