#
FRONT POWER WINDOW REGULATOR DISASSEMBLY/ASSEMBLY

BME091258560W02

  Caution

  • The automatic window return may not operate properly if the frame of the driver-side front power window regulator is removed from the power window motor. After performing any work, be sure to reset the power window motor. (See DRIVER-SIDE POWER WINDOW MOTOR RESETTING.)

1. Disassemble in the order indicated in the table.

2. Assemble in the reverse order of disassembly.

1 | Bolt
2 | Power window motor (See Power Window Motor Disassembly Note.)
3 | Frame

## Power Window Motor Disassembly Note

1. Hold the drum and the cable with the bracket to prevent them from being pulled out with the power window motor.