#
REAR AIR MIX ACTUATOR INSPECTION

BME074061415202

1. Remove the rear air mix actuator.

2. Connect battery positive voltage to terminal G and ground to terminal F, and battery positive voltage to terminal F and ground to terminal G of the rear air mix actuator.

3. Verify that the rear air mix actuator operates as shown below.

Connection | Movement
--- | ---
B+ | GND
F | G | HOT→COLD
G | F | COLD→HOT

4. Verify that the resistance between the terminals of the rear air mix actuator is as shown in the graph.

  • If not as specified, replace the rear air mix actuator.