#
POWER SLIDING DOOR (PSD) SYSTEM TERMINAL LAYOUT AND SIGNALS

BME090373001202

Terminal | Signal
--- | ---
| 1A | Easy closure control module (easy closure motor: close)
1B | Easy closure control module (easy closure motor: open)
1C | B+
1D | GND (signal)
2A | GND (power)
2B | PSD drive module (brake solenoid)
2D | PSD drive module (PSD motor: open)
2F | Door ajar warning light
2G | PSD drive module (PSD motor: close)
2H | Latch release actuator
| 3A | IG1
3B | Meter (speed)
3C | -
3D | Brake switch
3E | PSD front switch
3F | -
3G | PSD front switch (main switch)
3H | Easy closure control module (latch position switch)
3I | P position switch
3J | Rear door switch (RH or LH)
3K | PSD drive module (check switch)
3L | PSD drive module (speed sensor: pulse B)
3M | Parking brake switch
3N | PSD drive module (speed sensor: pulse A)
3O | Lock link switch
3P | Keyless control module
3Q | B+ (main)
3R | PSD rear switch (RH or LH)
3S | PSD front switch (RH or LH)
3T | -
3U | ABS warning light (Instrument cluster)
3V | -
3W | PSD drive module (speed sensor: power)
3X | PSD drive module (speed sensor: GND)