#
BRAKE SPECIFICATIONS

BME040000000T03

Item | Specification
--- | ---
Brake pedal | Type | Suspended
Pedal lever ratio | 4.1
Max. stroke | (mm {in}) | 125 {4.92}
Master cylinder | Type | Tandem (with level sensor)
Cylinder diameter | (mm {in}) | 23.81 {0.9374}
Front disc brake | Type | Ventilated disc
Cylinder bore | (mm {in}) | 42.85 {1.687} × 2
Pad dimensions (area × thickness) | 5,850 {9.36} × 10.5 {0.413}
(mm2 {in2} × mm {in})
Disc plate dimensions (outer diameter × thickness) | L3: 274 {10.8} × 28 {1.1} MZR-CD (RF Turbo): 296 {11.7} × 28 {1.1}
(mm {in})
Rear drum brake | Type | Leading-trailing
Wheel cylinder bore | (mm {in}) | L.H.D.:19.05 {0.75} R.H.D.: 20.64 {0.81}
Lining dimensions (area × length × thickness) | 50 × 203.8 × 4.5 {1.97 × 8.02 ×0.18}
(mm {in})
Drum inner diameter | (mm {in}) | 254 {10.0}
Shoe clearance adjustment | Automatic adjuster
Power brake unit | Type | Vacuum multiplier
Diameter | (mm {in}) | 293 {11.5}
Parking brake | Type | Mechanical two-rear-wheel control
Operation system | Center lever
Braking force control device | Type | Electronic Brakeforce Distribution (EBD)
Brake fluid | Type | SAE J1703, FMVSS116 DOT-3 or DOT-4