#
STEERING SPECIFICATIONS

BME060000000T03

Item | Specification
--- | ---
Engine | L3 | AJ | MZR-CD (RF Turbo)
Steering wheel | Outer diameter | (mm {in}) | 380 {15.0}
Lock-to-lock | (turn) | 3.3
Steering gear | Type | Rack-and-pinion
Rack stroke | (mm {in}) | 147.2 {5.8}
Steering shaft and joint | Shaft type | Collapsible
Joint type | 2-cross joint
Power steering | Power assist type | Engine speed sensing
Power steering fluid | Type | ATF M-III or equivalent (e.g. Dexron®II)
Capacity* (approximate quantity) | L.H.D.: 1.09 {1.15, 0.96} R.H.D.: 1.04 {1.10, 0.92} | L.H.D.: 1.05 {1.11, 0.92} R.H.D.: 1.00 {1.06, 0.88} | L.H.D.: 0.96 {1.01, 0.84} R.H.D.: 0.90 {0.95, 0.79}
(L {US qt, lmp qt})

  *
When reservoir tank is at maximum volume