#
NO.21 NOISE OCCURS AT IDLE WHEN VEHICLE IS STOPPED IN D, S, L RANGES, OR IN R POSITION [JA5A-EL]

BME050301030257

21 | Noise occurs at idle when vehicle is stopped in D, S, L ranges, or in R position
DESCRIPTION | • Transaxle noisy in driving ranges when vehicle idling.
POSSIBLE CAUSE | • Although the malfunction is basically the same as No.20 "NOISE OCCURS AT IDLE WHEN VEHICLE IS STOPPED IN ALL POSITIONS/RANGES", other causes may include selector lever position disparity or TR switch position disparity.

  Note

  • Before following the troubleshooting steps, make sure that the Automatic Transaxle On-Board Diagnostic and Automatic Transaxle Basic Inspection are conducted.