#
ABBREVIATIONS

BME000000000W10

A/C | Air conditioner
ABS | Antilock Brake System
ACC | Accessories
ATF | Automatic Transaxle Fluid
ATX | Automatic Transaxle
CAN | Controller Area Network
CCM | Comprehensive Component Monitor
CM | Control Module
DC | Drive Cycle
DEI | Double Electric Ignition
DLC-2 | Data link connector-2
DTC | Diagnostic Trouble Code
E/L | Electric Load
EX | Exhaust
FFD | Freeze Frame Data
GPS | Global Positioning System
HI | High
HU | Hydraulic Unit
IDM | Injector Driver Module
IG | Ignition
IN | Intake
INT | Intermittent
KOEO | Key On Engine Off
KOER | Key On Engine Running
LCD | Liquid Crystal Display
LF | Left Front
LH | Left Hand
LO | Low
L/R | Leading Rear
LR | Left Rear
M | Motor
MAX | Maximum
MIN | Minimum
MTX | Manual Transaxle
P/S | Power Steering
PCV | Positive Crankcase Ventilation
PID | Parameter Identification
PRC | Pressure Regulator Control
PSD | Power Sliding door
RDS | Radio Data System
RF | Right Front
RH | Right Hand
RPM | Engine Speed
RR | Right Rear
SAS | Sophisticated Air Bag Sensor
SST | Special Service Tool
SW | Switch
TCS | Traction Control System
TFT | Transaxle Fluid Temperature
TNS | Tail Number Side Lights
VBC | Variable Boost Control
VENT | Ventilation
VSC | Variable Swirl Control
VIS | Variable Intake-Air system
VTCS | Variable Tumble Control System
WDS | Worldwide Diagnostic System
1GR | First Gear
2GR | Second Gear