#
WINDSHIELD WIPER MOTOR INSPECTION

BME091967340202

1. Disconnect the windshield wiper motor connector.

2. Connect battery positive voltage to terminal D or C and ground to terminal F, and inspect the operation of the windshield wiper motor as indicated below.

Terminal | Operation
--- | ---
D | Low
C | High

3. Disconnect battery positive voltage from terminal C of the motor while the wipers are operating.

4. Verify that the wipers do not stop in the park position.

5. Short between the motor terminals B and D and connect battery positive voltage to the motor terminal A.

6. Verify that the wipers operate at low speed again, then stop in the park position.

  • If not as specified, replace the windshield wiper motor.