#
FRONT DOOR TRIM REMOVAL/INSTALLATION

BME091768420W01

1. Disconnect the negative battery cable if equipped with power window system.

2. Remove the inner garnish.

3. Remove the regulator handle if equipped.

4. Remove the fasteners.

5. Remove the cover.

6. Remove screw A.

7. Remove screw B.

8. Remove the lens.

9. Remove screw C.

10. Disengage clips D from the body using a fastener remover.

11. Pull the front door trim upward, then disengage hooks E from the body.

12. Extract the inner handle from the front door trim.

13. Disconnect the door lock switch connector and the power window main switch connector if equipped. (driver's side)

14. Disconnect the power window subswitch connector if equipped. (passenger's side)

15. Remove the courtesy light.

16. Remove the front door trim.

17. Install in the reverse order of removal.