#
AUTOMATIC TRANSAXLE LOCATION INDEX [JA5A-EL]

BME051701030203

1 | HOLD switch (See HOLD SWITCH INSPECTION [JA5A-EL].) (See HOLD SWITCH REMOVAL/INSTALLATION [JA5A-EL].)
2 | TR switch (See TRANSAXLE RANGE (TR) SWITCH INSPECTION [JA5A-EL].) (See TRANSAXLE RANGE (TR) SWITCH REMOVAL/INSTALLATION [JA5A-EL].) (See TRANSAXLE RANGE (TR) SWITCH ADJUSTMENT [JA5A-EL].)
3 | TFT sensor (See TRANSAXLE FLUID TEMPERATURE (TFT) SENSOR REMOVAL/INSTALLATION [JA5A-EL].) (See TRANSAXLE FLUID TEMPERATURE (TFT) SENSOR INSPECTION [JA5A-EL].)
4 | Vehicle speed sensor (See VEHICLE SPEED SENSOR (VSS) REMOVAL/INSTALLATION [JA5A-EL].) (See VEHICLE SPEED SENSOR (VSS) INSPECTION [JA5A-EL].)
5 | Intermediate sensor (See INTERMEDIATE SENSOR REMOVAL/INSTALLATION [JA5A-EL].) (See INTERMEDIATE SENSOR INSPECTION [JA5A-EL].)
6 | Input/turbine speed sensor (See INPUT/TURBINE SPEED SENSOR INSPECTION [JA5A-EL].) (See INPUT/TURBINE SPEED SENSOR REMOVAL/INSTALLATION [JA5A-EL].)
7 | Solenoid valve (See SOLENOID VALVE INSPECTION [JA5A-EL].) (See SOLENOID VALVE REMOVAL/INSTALLATION [JA5A-EL].)
8 | HOLD indicator light (See HOLD INDICATOR LIGHT INSPECTION [JA5A-EL].)
9 | TCM (See TCM INSPECTION [JA5A-EL] (VIN: JMZ LW19J7*# 300001-, JM0 LW10J300 300001-301405, JM6 LW10J300 300001-, JM8 LW28J**# 300001-301513).) (See TCM INSPECTION [JA5A-EL] (VIN: JM0 LW10J300 301406-, JMZ LW69J7*# 307683-, JM8 LW28J**# 301514-, JM8 LW28A**# 301514- (Assumed)).)
(See TCM REMOVAL/INSTALLATION [JA5A-EL].)
10 | Transaxle (See AUTOMATIC TRANSAXLE REMOVAL/INSTALLATION [JA5A-EL].)
11 | Control valve body (See CONTROL VALVE BODY REMOVAL/INSTALLATION [JA5A-EL].)
12 | Oil cooler (See OIL COOLER FLUSHING [JA5A-EL].) (See OIL COOLER REMOVAL/INSTALLATION [JA5A-EL].) (See OIL COOLER DISASSEMBLY/ASSEMBLY [JA5A-EL].)
13 | Drive plate (See DRIVE PLATE REMOVAL/INSTALLATION [JA5A-EL].)