#
BRAKE PIPE JOINT REPLACEMENT

BME041143900201

1. For the AJ engine model, remove the dynamic chamber. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [AJ].)

2. For the MZR-CD (RF Turbo) engine model, remove the heater hose. (See HEATER PIPE AND HOSE COMPONENT REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

1 | Brake pipe
2 | Bolt
3 | Brake pipe joint (See Brake Pipe Joint Installation Note)

4. Install in the reverse order of removal.

## Brake Pipe Joint Installation Note

1. Install the Brake pipe joint so that the R mark faces the left side of the vehicle.