#
DOOR KEY CYLINDER SWITCH INSPECTION

BME091475911202

1. Fully raise the door glass.

2. Disconnect the negative battery cable.

3. Remove the front door trim.

4. Turn the door screen over.

5. Disconnect the door key cylinder switch connector.

6. Inspect for continuity between the door key cylinder switch terminals using an ohmmeter.

  • If not as specified, replace the door key cylinder switch.