#
AUTOMATIC TRANSAXLE ON-BOARD DIAGNOSTIC FUNCTION [JA5A-EL]

BME050218901202

## DTC Reading Procedure

### Using the WDS or equivalent

1. Perform the necessary vehicle preparation and visual inspection.

2. Connect the WDS or equivalent to the vehicle DLC-2 16-pin connector located the left side of the center console.

3. Retrieve the DTCs using the WDS or equivalent.

### Using the voltmeter

1. Turn the ignition switch to the LOCK position.

2. Connect the DLC located in transaxle compartment terminal TAT and ground using a jumper wire.

  Caution

  • Connecting to the wrong DLC terminal may cause a malfunction. Carefully connect only to the specified terminal.

3. Connect the negative battery lead of voltmeter (20 V range) to data link connector terminal FAT, and the positive lead to the data link connector terminal B+.

4. Turn the ignition switch to the ON position.

5. The voltmeter indicates the battery positive voltage for approx. 3 s, then indicates 0 V.

6. Read the DTCs indicated by the movement of the voltmeter needle. If DTC is not detected, the needle does not move.

  Note

  • Code No. indication by the voltmeter needle is as shown.

7. If any DTCs is indicated, inspect the appropriate area and repair it necessary.