#
DTC P0703 [L3]

BME010200700W01

DTC P0703 | Brake switch input malfunction
--- | ---
DETECTION CONDITION | • PCM monitors changes in input voltage from brake switch. If PCM does not detect PCM terminal 1K voltage changes while alternately accelerating and decelerating 10 times, PCM determines that neutral switch circuit has malfunction. Diagnostic support note
• This is a continuous monitor (CCM).
• MIL illuminates if PCM detects the above malfunction condition in two consecutive drive cycles or in one drive cycle while the DTC for the same malfunction has been stored in the PCM.
• PENDING CODE is available if PCM detects the above malfunction condition during first drive cycle.
• FREEZE FRAME DATA is available.
• DTC is stored in PCM memory.
POSSIBLE CAUSE | • Brake switch malfunction • Poor connection of brake switch connector or PCM connector • Short to power between brake switch terminal B and PCM connector terminal 1K • Open harness between brake switch terminal B and PCM connector terminal 1K • Open harness between battery positive terminal and brake switch terminal A
• PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA HAS BEEN RECORDED • Has FREEZE FRAME DATA been recorded? | Yes | Go to next step.
No | Record FREEZE FRAME DATA on repair order, then go to next step.
2 | VERIFY RELATED SERVICE INFORMATION AVAILABILITY • Check for related Service Information availability. • Is any related Service Information available? | Yes | Perform repair or diagnosis according to available Service Information. • If vehicle is not repaired, go to next step.
No | Go to next step.
3 | CLASSIFY HIGH INPUT OR LOW INPUT • Connect WDS or equivalent to DLC-2. • Access BOO PID. • Verify BOO PID during brake pedal operation. • Is BOO PID always OFF? | Yes | Go to Next step.
No | Go to Step 10.
4 | INSPECT BRAKE SWITCH CONNECTOR FOR POOR CONNECTION • Turn ignition switch to OFF. • Disconnect brake switch connector. • Inspect for poor connection (damaged/pulled-out terminals, corrosion, etc.). • Is there any malfunction? | Yes | Repair or replace terminal, then go to Step 14.
No | Go to next step.
5 | CLASSIFY BRAKE SWITCH OR CIRCUIT • Connect WDS or equivalent to DLC-2. • Access BOO PID. • Connect a jumper wire between brake switch terminal A and B. • Is BOO PID on? | Yes | Go to next step.
No | Go to Step 7.
6 | INSPECT BRAKE SWITCH • Perform brake switch inspection. • Is brake switch okay? | Yes | Go to Step 14.
No | Replace brake switch, then go to Step 14.
7 | INSPECT BRAKE SWITCH POWER CIRCUIT FOR OPEN CIRCUIT • Measure voltage between brake switch connector terminal A and body ground. • Is voltage B+? | Yes | Go to next step.
No | Repair or replace brake switch power circuit for open, then Go to Step 14.
8 | INSPECT PCM CONNECTOR FOR POOR CONNECTION • Turn ignition switch to OFF. • Disconnect PCM connector. • Inspect for poor connection (damaged/pulled-out terminals, corrosion, etc.). • Is there any malfunction? | Yes | Repair or replace terminal, then go to Step 14.
No | Go to next step.
9 | INSPECT BRAKE SWITCH SIGNAL CIRCUIT FOR OPEN CIRCUIT • Inspect continuity between brake switch terminal B and PCM terminal 1K. • Is there continuity? | Yes | Repair or replace harness for open, then go to Step 14.
No | Go to Step 14.
10 | INSPECT BRAKE SWITCH CONNECTOR FOR POOR CONNECTION • Turn ignition switch to OFF. • Disconnect brake switch connector. • Inspect for poor connection (damaged/pulled-out terminals, corrosion, etc.). • Is there any malfunction? | Yes | Repair or replace terminal, then go to Step 14.
No | Go to next step.
11 | CLASSIFY BRAKE SWITCH OR CIRCUIT • Connect WDS or equivalent to DLC-2. • Access BOO PID. • Verify that BOO PID changes from ON to OFF when brake switch connector disconnected. • Does BOO PID change from ON to OFF? | Yes | Go to next step.
No | Go to Step 13.
12 | INSPECT BRAKE SWITCH • Perform brake switch inspection. • Is brake switch okay? | Yes | Go to Step 14.
No | Replace brake switch, then go to Step 14.
13 | INSPECT BRAKE SWITCH SIGNAL CIRCUIT FOR SHORT TO POWER • Measure voltage between brake switch connector terminal B and body ground. • Is voltage B+? | Yes | Repair or replace harness for short to power, then go to Step 14.
No | Go to next step.
14 | VERIFY TROUBLESHOOTING OF DTC P0703 COMPLETED • Make sure to reconnect all disconnected connectors. • Clear DTC from memory using WDS or equivalent. • Drive vehicle 30 km/h {18.6 mph} or more. • Depress and release brake pedal more than 10 times while driving vehicle.
• Is PENDING CODE of same DTC present?
Yes
Replace PCM, then go to next step.
(See PCM REMOVAL/INSTALLATION [L3].)
No | Go to next step.
15 | VERIFY AFTER REPAIR PROCEDURE • Perform "After Repair Procedure". (See AFTER REPAIR PROCEDURE [L3].) • Is there DTC present? | Yes | Go to applicable DTC troubleshooting. (See DTC TABLE [L3].)
No | Troubleshooting completed.