#
INSTRUMENT CLUSTER SYSTEM SPECIFICATIONS

BME092200000T05

Item | Specification
--- | ---
Speedometer | Meter type | Cross coil type
Indication range | European (L.H.D.) General (L.H.D.) Australian specs. (km/h) | 0-210
UK specs. (km/h {MPH}) | 0-210 {0-130}
General (R.H.D.) specs. (km/h) | 0-180
Input signal source | With ABS and TCS | ABS/TCS HU/CM
With ABS, Without TCS | ABS HU/CM
Input signal | 8 pulses/one rotation of speedometer driven gear
Output signal | 4 pulses/one rotation of speedometer driven gear
Rated voltage (V) | DC 12
Tachometer | Meter type | Cross coil type
Indication range (rpm) | 0-8000
Red zone (rpm) | 6700-8000
Input signal source | PCM
Input signal | 6 pulses/two engine rotations
Rated voltage (V) | DC 12
Fuel gauge | Meter type | Cross coil type (Indicator needle type)
Rated voltage (V) | DC 12
Water temperature gauge | Meter type | Cross coil type (Medium range stabilized type)
Rated voltage (V) | DC 12
Odometer | Display | Liquid crystal display
Indication digits | 6 digits
Characteristics | 1 km is added for 5096 pulses of vehicle speed input signal 1 mile is added for 8202 pulses of vehicle speed input signal
Rated voltage (V) | DC 12
Tripmeter | Display | Liquid crystal display
Indication digits | 4 digits
Cancellation | Push method
Characteristics | 1 km is added for 5096 pulses of vehicle speed input signal 1 mile is added for 8202 pulses of vehicle speed input signal
Rated voltage (V) | DC 12