#
WHEEL HUB BOLT REPLACEMENT

BME031133060201

1. Remove the hub bolt using the SST.

  Note

  • If the dust cover interferes with the wheel hub bolt and the wheel hub bolt cannot be removed. Tap the part shown in the figure with a chisel lightly and bend the processing point back to the steering knuckle side.

2. Install the hub bolt into the wheel hub and install a washer and hub nut on the hub bolt.

3. Tighten the hub nut while holding the wheel hub using a brass bar.