#
REAR BRAKE (DRUM) REMOVAL/INSTALLATION

BME041126250W02

1. Remove in the order indicated in the table.

2. Install in the reverse order of removal.

3. After installation, do the following.

  (1) Depress the brake pedal a few times. Then verify that the brakes do not drag.
  (2) Inspect the pedal-to-floor clearance.
  (3) Inspect the parking brake lever stroke.

.

1 | Hub cap
2 | Screw
3 | Brake drum (See Brake Drum Removal Note) (See Brake Drum Installation Note)
4 | Return spring
5 | Hold pin and hold spring
6 | Anti-rattle spring
7 | Leading shoe
8 | Parking brake cable
9 | Trailing shoe
10 | Ajuster lever
11 | Adjuster component
12 | Operating lever
13 | Brake pipe
14 | Wheel cylinder
15 | O-ring
16 | Locknut (See Locknut Removal Note) (See Locknut Installation Note)
17 | Wheel hub
18 | Backing plate

## Brake Drum Removal Note

1. Mark the wheel hub bolt and brake drum before removal for reference during installation.

## Brake Drum Installation Note

### Using auto adjuster

1. When installing the brake drum, adjust the brake shoe clearance as described below.

  (1) Turn the adjuster on the adjust strust so that the length (L) is 2 mm-3 mm {0.079 in-0.11 in}.
  (2) Remove any rust or grime on the contact face of the drum brake.
  (3) Install the brake drum and align the marks made before removal.
  (4) Depress the brake pedal thirty times to operate the auto adjuster.