#
PRECAUTION (STEERING)

BME061001034201

## Wheels and Tires Removal/Installation

1. The removal and installation procedures for the wheels and tires are not mentioned in this section. When a wheel is removed, tighten it to 107.8-147.0 N·m {11.00-14.98 kgf·m, 79.6-108.4 ft·lbf}.

## Power Steering Components Removal/Installation

1. If any power steering fluid line has been disconnected anytime during the procedure, add ATF M-III or equivalent (e.g. Dexron®III), bleed the fluid lines, and inspect for leakage after the procedure has been completed.

## Connectors Disconnection/Connection

1. Disconnect the negative battery cable before performing any work that requires handling of connectors. Reconnect the negative battery cable only after the work is completed.