#
TRANSAXLE FLUID TEMPERATURE (TFT) SENSOR REMOVAL/INSTALLATION [JA5A-EL]

BME051719010201

1. Remove the automatic transaxle. (See AUTOMATIC TRANSAXLE REMOVAL/INSTALLATION [JA5A-EL].)

2. Disassemble the automatic transaxle, and then remove the TFT sensor. (See Automatic Transaxle Workshop Manual JA5A-EL)

3. Install a TFT sensor, and then assemble the automatic transaxle. (See Automatic Transaxle Workshop Manual JA5A-EL)

4. Remove the automatic transaxle. (See AUTOMATIC TRANSAXLE REMOVAL/INSTALLATION [JA5A-EL].)

5. Perform the line pressure test. (See Line Pressure Test.)

6. Inspect the operation of the TR switch. (See TRANSAXLE RANGE (TR) SWITCH INSPECTION [JA5A-EL].)

7. Inspect the operation of the selector lever. (See SELECTOR LEVER INSPECTION.)

8. Perform the mechanical system test. (See MECHANICAL SYSTEM TEST [JA5A-EL].)