#
DTC TABLE [FN4A-EL]

BME050201030204

DTC No. | Condition | MIL | HOLD indicator light flashes | DC | Monitor item | Memory function | Page
--- | --- | --- | --- | --- | --- | --- | ---
P0031 | Front HO2S heater circuit low input | (See DTC TABLE [L3].)
P0032 | Front HO2S heater circuit high input | (See DTC TABLE [L3].)
P0037 | Rear HO2S heater circuit low input | (See DTC TABLE [L3].)
P0038 | Rear HO2S heater circuit high input | (See DTC TABLE [L3].)
P0101 | MAF sensor inconsistent with TP sensor | (See DTC TABLE [L3].)
P0102 | MAF circuit low input | (See DTC TABLE [L3].)
P0103 | MAF circuit high input | (See DTC TABLE [L3].)
P0107 | MAP sensor circuit low input | (See DTC TABLE [L3].)
P0108 | MAP sensor circuit high input | (See DTC TABLE [L3].)
P0111 | IAT circuit performance problem | (See DTC TABLE [L3].)
P0112 | IAT circuit low input | (See DTC TABLE [L3].)
P0113 | IAT circuit high input | (See DTC TABLE [L3].)
P0117 | ECT circuit low input | (See DTC TABLE [L3].)
P0118 | ECT circuit high input | (See DTC TABLE [L3].)
P0121 | Throttle position stuck closed | (See DTC TABLE [L3].)
P0122 | TP circuit low input | (See DTC TABLE [L3].)
P0123 | TP circuit high input | (See DTC TABLE [L3].)
P0125 | Excessive time to enter closed loop fuel control | (See DTC TABLE [L3].)
P0131 | Front HO2S no inversion (low stuck) | (See DTC TABLE [L3].)
P0132 | Front HO2S no inversion (high stuck) | (See DTC TABLE [L3].)
P0133 | Front HO2S circuit malfunction | (See DTC TABLE [L3].)
P0134 | Front HO2S circuit no activity detected | (See DTC TABLE [L3].)
P0138 | Rear HO2S circuit high input | (See DTC TABLE [L3].)
P0140 | Rear HO2S circuit no activity detected | (See DTC TABLE [L3].)
P0171 | Fuel trim system too lean | (See DTC TABLE [L3].)
P0172 | Fuel trim system too rich | (See DTC TABLE [L3].)
P0300 | Random misfire detected | (See DTC TABLE [L3].)
P0301 | Cylinder No.1 misfire detected | (See DTC TABLE [L3].)
P0302 | Cylinder No.2 misfire detected | (See DTC TABLE [L3].)
P0303 | Cylinder No.3 misfire detected | (See DTC TABLE [L3].)
P0304 | Cylinder No.4 misfire detected | (See DTC TABLE [L3].)
P0327 | Knock sensor circuit low input | (See DTC TABLE [L3].)
P0328 | Knock sensor circuit high input | (See DTC TABLE [L3].)
P0335 | CKP sensor circuit malfunction | (See DTC TABLE [L3].)
P0340 | CMP sensor circuit malfunction | (See DTC TABLE [L3].)
P0403 | EGR valve motor coils open or short | (See DTC TABLE [L3].)
P0420 | Catalyst system efficiency below threshold | (See DTC TABLE [L3].)
P0443 | Evaporative emission control system purge control valve circuit malfunction | (See DTC TABLE [L3].)
P0480 | Fan control module circuit malfunction | (See DTC TABLE [L3].)
P0500 | VSS circuit malfunction (MTX) | (See DTC TABLE [L3].)
VSS circuit malfunction (ATX) | ON | YES | 2 | CCM | X | (See DTC P0500 [FN4A-EL])
P0505 | Idle control system malfunction | (See DTC TABLE [L3].)
P0506 | Idle control system RPM lower than expected | (See DTC TABLE [L3].)
P0507 | Idle control system RPM higher than expected | (See DTC TABLE [L3].)
P0511 | IAC valve circuit malfunction | (See DTC TABLE [L3].)
P0550 | PSP switch circuit malfunction | (See DTC TABLE [L3].)
P0661 | VIS control circuit low input | (See DTC TABLE [L3].)
P0662 | VIS control circuit high input | (See DTC TABLE [L3].)
P0703 | Brake switch input malfunction | (See DTC TABLE [L3].)
P0704 | Clutch switch input malfunction | (See DTC TABLE [L3].)
P0705 | Transaxle range (TR) switch circuit malfunction (short circuit) | ON | YES | 2 | CCM | X | (See DTC P0705 [FN4A-EL])
P0706 | Transaxle range (TR) switch circuit malfunction (open circuit) | ON | YES | 2 | CCM | X | (See DTC P0706 [FN4A-EL])
P0711 | Transaxle fluid temperature (TFT) sensor circuit range/performance (stuck) | ON | NO | 2 | CCM | X | (See DTC P0711 [FN4A-EL])
P0712 | Transaxle fluid temperature (TFT) sensor circuit malfunction (short to ground) | ON | YES | 1 | CCM | X | (See DTC P0712 [FN4A-EL])
P0713 | Transaxle fluid temperature (TFT) sensor circuit malfunction (open circuit) | ON | YES | 1 | CCM | X | (See DTC P0713 [FN4A-EL])
P0715 | Input/turbine speed sensor circuit malfunction | ON | YES | 1 | CCM | X | (See DTC P0715 [FN4A-EL])
P0731 | Gear 1 incorrect (incorrect gear ratio detected) | OFF | YES | 1 | CCM | X | (See DTC P0731 [FN4A-EL])
P0732 | Gear 2 incorrect (incorrect gear ratio detected) | OFF | YES | 1 | CCM | X | (See DTC P0732 [FN4A-EL])
P0733 | Gear 3 incorrect (incorrect gear ratio detected) | OFF | YES | 1 | CCM | X | (See DTC P0733 [FN4A-EL])
P0734 | Gear 4 incorrect (incorrect gear ratio detected) | OFF | YES | 1 | CCM | X | (See DTC P0734 [FN4A-EL])
P0741 | Torque converter clutch (TCC) (stuck OFF) | OFF | YES | 1 | CCM | X | (See DTC P0741 [FN4A-EL])
P0742 | Torque converter clutch (TCC) (stuck ON) | OFF | YES | 1 | CCM | X | (See DTC P0742 [FN4A-EL])
P0745 | Pressure control solenoid malfunction | OFF | YES | 1 | CCM | X | (See DTC P0745 [FN4A-EL])
P0751 | Shift solenoid A stuck OFF | ON | YES | 2 | CCM | X | (See DTC P0751 [FN4A-EL])
P0752 | Shift solenoid A stuck ON | ON | YES | 2 | CCM | X | (See DTC P0752 [FN4A-EL])
P0753 | Shift solenoid A malfunction (electrical) | ON | YES | 1 | CCM | X | (See DTC P0753 [FN4A-EL])
P0756 | Shift solenoid B stuck OFF | ON | YES | 2 | CCM | X | (See DTC P0756 [FN4A-EL])
P0757 | Shift solenoid B stuck ON | ON | YES | 2 | CCM | X | (See DTC P0757 [FN4A-EL])
P0758 | Shift solenoid B malfunction (electrical) | ON | YES | 1 | CCM | X | (See DTC P0758 [FN4A-EL])
P0761 | Shift solenoid C stuck OFF | ON | YES | 2 | CCM | X | (See DTC P0761 [FN4A-EL])
P0762 | Shift solenoid C stuck ON | ON | YES | 2 | CCM | X | (See DTC P0762 [FN4A-EL])
P0763 | Shift solenoid C malfunction (electrical) | ON | YES | 1 | CCM | X | (See DTC P0763 [FN4A-EL])
P0766 | Shift solenoid D stuck OFF | ON | YES | 2 | CCM | X | (See DTC P0766 [FN4A-EL])
P0767 | Shift solenoid D stuck ON | ON | YES | 2 | CCM | X | (See DTC P0767 [FN4A-EL])
P0768 | Shift solenoid D malfunction (electrical) | ON | YES | 1 | CCM | X | (See DTC P0768 [FN4A-EL])
P0771 | Shift solenoid E stuck OFF | ON | YES | 2 | CCM | X | (See DTC P0771 [FN4A-EL])
P0772 | Shift solenoid E stuck ON | ON | YES | 2 | CCM | X | (See DTC P0772 [FN4A-EL])
P0773 | Shift solenoid E malfunction (electrical) | ON | YES | 1 | CCM | X | (See DTC P0773 [FN4A-EL])
P0841 | Oil pressure switch circuit malfunction | OFF | NO | 2 | CCM | X | (See DTC P0841 [FN4A-EL])
P0894 | Forward clutch torque transmission | OFF | YES | 1 | CCM | X | (See DTC P0894 [FN4A-EL].)
P0850 | Neutral switch input malfunction | (See DTC TABLE [L3].)
P1562 | PCM +BB voltage low | (See DTC TABLE [L3].)
P1602 | Immobilizer unit-PCM communication error | (See DTC TABLE [L3].)
P1603 | Key ID numbers are not registered in PCM | (See DTC TABLE [L3].)
P1604 | Code word is not registered in PCM | (See DTC TABLE [L3].)
P1621 | Code word does not match after engine cranking | (See DTC TABLE [L3].)
P1622 | Key ID number does not match | (See DTC TABLE [L3].)
P1623 | Code word or key ID number read/write error in PCM | (See DTC TABLE [L3].)
P1624 | Immobilizer system communication counter=0 | (See DTC TABLE [L3].)
P2006 | VTCS shutter valve stuck closed | (See DTC TABLE [L3].)
P2009 | Variable tumble control solenoid circuit low input | (See DTC TABLE [L3].)
P2010 | Variable tumble control solenoid circuit high input | (See DTC TABLE [L3].)
P2228 | BARO sensor circuit low input | (See DTC TABLE [L3].)
P2229 | BARO sensor circuit high input | (See DTC TABLE [L3].)
P2502 | Generator output voltage signal no electricity | (See DTC TABLE [L3].)
P2503 | Battery overcharge | (See DTC TABLE [L3].)
P2504 | Generator terminal B circuit open | (See DTC TABLE [L3].)