#
WATER HEATER UNIT REMOVAL/INSTALLATION

BME074000170W01

## L.H.D.

1. Complete the "BEFORE REPAIR PROCEDURE". (See BEFORE REPAIR PROCEDURE [MZR-CD (RF Turbo)].)

2. Disconnect the negative battery cable.

3. Drain the engine coolant.

4. To remove the exhaust pipe, remove the front stabilizer.

5. Remove in the order indicated in the table.

6. Install in the reverse order of removal.

7. Complete the "AFTER REPAIR PROCEDURE". (See AFTER REPAIR PROCEDURE [MZR-CD (RF Turbo)].)

8. Refill the engine coolant.

1 | Connector
2 | Heater hose No.5
3 | Heater hose No.4
4 | Water heater unit
5 | Exhaust pipe

## R.H.D.

1. Complete the "BEFORE REPAIR PROCEDURE". (See BEFORE REPAIR PROCEDURE [MZR-CD (RF Turbo)].)

2. Disconnect the negative battery cable.

3. Drain the engine coolant.

4. Remove the battery.

5. Remove the air cleaner.

6. Remove the fuel filter body with the pipes still connected, and fix the fuel filter body using a rope so that it is out of the way.

7. Remove in the order indicated in the table.

8. Install in the reverse order of removal.

9. Complete the "AFTER REPAIR PROCEDURE". (See AFTER REPAIR PROCEDURE [MZR-CD (RF Turbo)].)

10. Refill the engine coolant.

1 | Connector
2 | Heater hose No.5
3 | Heater hose No.4
4 | Water heater unit
5 | Exhaust pipe