#
OIL FILTER REPLACEMENT [MZR-CD (RF Turbo)]

BME011114300W03

  Warning

  • Continuous exposure with USED engine oil has caused skin cancer in laboratory mice. Protect your skin by washing with soap and water immediately after this work.
  • Hot engines and engine oil can cause severe burns. Turn off the engine and wait until it and the engine oil have cooled.

1. Remove the oil filter using the filter wrench.

2. Use a clean rag to wipe off the mounting surface on the oil filter.

3. Apply clean engine oil to the O-ring of the new oil filter.

4. Using the filter wrench, tighten the filter according to the installation procedure indicated on the side of the filter or packing box.

5. Start the engine and inspect for oil leakage.

  • If the oil leaks, specify the faulty part and repair or replace it.

6. Inspect the oil level.

  • If necessary, add oil. (See ENGINE OIL LEVEL INSPECTION.)