#
LIFTGATE ADJUSTMENT

BME091162010203

1. Measure the gap and height between the liftgate and the body.

2. If not as specified, loosen the liftgate hinge installation bolts or the liftgate striker installation screws, and reposition the liftgate.

Clearance

  a: 6.8-9.8 mm {0.27-0.38 in}
  b: -2.5-0 mm {-0.09-0 in}
  c: 3.3-7.7 mm {0.13-0.30 in}
  d: -3.0-1.0 mm {-0.11-0.03 in}
  e: 3.3-7.7 mm {0.13-0.30 in}
  f: -3.7-0.3 mm {-0.14-0.01 in}
  g: 4.5-9.5 mm {0.18-0.37 in}

3. Tighten the bolts or screws.