#
FRONT EVAPORATOR REMOVAL/INSTALLATION

BME071161010201

1. Disconnect the negative battery cable.

2. Evacuate the refrigerant from the system. (See REFRIGERANT CHARGING.)

3. sconnect the front cooler pipe No.3 from the expansion valve. (See FRONT A/C UNIT REMOVAL/INSTALLATION.)

4. Remove the glove compartment.

5. Slide the air duct toward (A) and push it down toward (B) to remove it.

6. Remove the PCM. (See PCM REMOVAL/INSTALLATION [L3].) (See PCM REMOVAL/INSTALLATION [AJ].)

7. Remove in the order indicated in the table.

8. Install in the reverse order of removal.

1 | Heater case (5)
2 | Cover
3 | Front evaporator