#
WATER PUMP REMOVAL/INSTALLATION [AJ]

BME011215010202

1. Remove the battery and battery tray. (See BATTERY REMOVAL/INSTALLATION [L3, AJ].)

2. Drain the engine coolant. (See COOLING SYSTEM SERVICE WARNINGS.)(See ENGINE COOLANT REPLACEMENT [AJ].)

3. Remove the water pump drive pulley. (See Water Pump Drive Belt Pulley Removal Note.)

4. Remove in the order indicated in the table.

5. Install in the reverse order of removal.

1 | Thermostat case
2 | Oil cooler hose
3 | Water outlet pipe
4 | Water pump (See Water Pump Installation Note.)

## Water Pump Installation Note

1. Tighten the bolts to the specified torque, then tighten them further 85-90.