#
JOINT SHAFT DISASSEMBLY/ASSEMBLY [L3]

BME031325700W05

1. Disassemble in the order indicated in the table.

2. Assemble in the reverse order of disassembly.

.

1 | Bolt
2 | Joint shaft (See Joint Shaft Disassembly Note.) (See Joint Shaft Assembly Note.)
3 | Dust cover
4 | Dust seal (differential side) (See Dust Seal (Differential Side), Bearing Disassembly Note.) (See Dust Seal (Differential Side) Assembly Note.)
5 | Bearing (See Dust Seal (Differential Side), Bearing Disassembly Note.) (See Bearing Assembly Note.)
6 | Dust seal (drive shaft side) (See Dust Seal (Drive Shaft Side) Disassembly Note.) (See Dust Seal (Drive Shaft Side) Assembly Note.)
7 | Bracket

## Joint Shaft Disassembly Note

1. Loosen the dust cover installation bolt, and remove the dust cover from the bracket.

2. Disassemble the joint shaft using a bar and press.

## Dust Seal (Differential Side), Bearing Disassembly Note

1. Remove the dust seal (differential side) and bearing using the SSTs and a press.

## Dust Seal (Drive Shaft Side) Disassembly Note

1. Remove the dust seal (drive shaft side) using the SSTs and a press.

## Dust Seal (Drive Shaft Side) Assembly Note

1. Apply grease to the new dust seal lip.

2. Install the new dust seal (drive shaft side) using the SSTs and a press.

## Bearing Assembly Note

1. Install the new bearing using the SSTs.

## Dust Seal (Differential Side) Assembly Note

1. Apply grease to the new dust seal lip.

2. Install the new differential side dust seal using a steel plate, the SSTs and a press.

## Joint Shaft Assembly Note

1. Assemble the joint shaft using the SST and a press.