#
MASTER CYLINDER REMOVAL/INSTALLATION

BME041143400W04

1. For the MZR-CD (RF Turbo) engine model, remove the fuel filter installation bolt and put the fuel filter aside. (See FUEL FILTER COMPONENT REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

2. Remove in the order indicated in the table.

1 | Brake fluid level sensor connector
2 | Brake pipe
3 | Master cylinder (See Master Cylinder Installation Note)

3. Install in the reverse order of removal.

## Master Cylinder Installation Note

1. Place the SST atop the master cylinder. Turn the adjusting bolt until it touches the bottom of the push rod hole in the piston.

2. Apply 66.7 kPa {500 mmHg, 19.7 inHg} vacuum to the power brake unit using a vacuum pump.

3. Invert the SST used in step 1 and place it on the power brake unit.

4. Measure the clearance between the end of the SST and the push rod of the power brake unit.

  • If it is not 0 mm {0 in}, loosen the push rod locknut and turn the push rod to adjust it by using the SSTs.