#
DTC CONFIRMATION PROCEDURE [MZR-CD (RF Turbo)]

BME010200000W18

STEP | INSPECTION | ACTION
--- | --- | ---
1 | RECORD CONTINUOUS MEMORY DTC • Turn engine switch to ON (Engine OFF). • Retrieve all stored DTCs using WDS or equivalent. • Are there any DTCs present? | Yes | Record all stored DTCs (continuous memory DTC), then go to next step.
No | Go to next step.
2 | VERIFY RELATED REPAIR INFORMATION AVAILABILITY • Check for related Service Information availability. • Is any related repair information available? | Yes | Perform repair or diagnosis according to available Service information. • If vehicle is not repaired, go to next step.
No | Go to next step.
3 | PERFORM KOEO SELF-TEST • Start engine. • Warm up engine completely. • Turn off all electrical loads. • Perform KOEO SELF-TEST PROCEDURE.
(See KOEO/KOER SELF-TEST PROCEDURE [MZR-CD (RF Turbo)].)
• Are there any KOEO DTCs present?
Yes
Repair KOEO DTC.
(See DTC TABLE [MZR-CD (RF Turbo)].)
No | Go to next step.
4 | PERFORM KOER SELF-TEST • Start engine. • Perform KOER SELF-TEST PROCEDURE. (See KOEO/KOER SELF-TEST PROCEDURE [MZR-CD (RF Turbo)].) • Are there any KOER DTCs present? | Yes | Repair KOER DTC. (See DTC TABLE [MZR-CD (RF Turbo)].)
No | • If continuous memory DTC is present at Step 1, return to applicable DTC troubleshooting procedure step. • If continuous memory DTC is not present at Step 1, go to symptom troubleshooting.