#
DOOR OUTLINE

BME091101085T11
• The rear doors are of sliding design with three rails.
• Sliding door circuit contacts are installed on the sliding door and the body in order to supply electrical power to the sliding door.
• Side impact bars and sliding door catcher pins are used in the sliding doors to improve passenger safety in the event of a side collision.
• To prevent the sliding door from hitting the fuel-filler lid, the sliding door cannot be opened when the fuel-filler lid is open.
• The open lock that holds the door at fully open position has been adopted.
• A power sliding door (PSD) system, which allows the sliding doors to open/close automatically, has been adopted for both LH and RH sliding doors.