#
ACCELERATOR CABLE INSPECTION [L3]

BME011341660W01

1. Verify that the throttle valve is closed.

2. Push the cable into the housing without turning the throttle plate and put a white mark on the cable at the end of the housing.

3. Release the cable and measure the distance from the white mark to the end of the cable housing.

  • If not within the specification, adjust the accelerator cable. (See ACCELERATOR CABLE ADJUSTMENT [L3].)

Free play

  1.5-4.0 mm {0.06-0.15 in}