#
AFTER SERVICE PRECAUTION [AJ]

BME011400114213

  Warning

  • Fuel line spills and leakage are dangerous. Fuel can ignite and cause serious injuries or death and damage. When installing the fuel hose, observe "Fuel Leakage Inspection" described below.

## Fuel Leakage Inspection

  Warning

  • Fuel line spills and leakage are dangerous. Fuel can ignite and cause serious injuries or death and damage. Always carry out the following procedure with the engine stopped.

  Caution

  • Connecting the wrong DLC terminal may possibly cause a malfunction. Carefully connect the specified terminal only.

1. Short the DLC terminal F/P to body GND using a jumper wire.

2. Turn the ignition switch to ON position to operate the fuel pump.

3. Pressurize the system this way for at least 5 min to be sure of no leakage.

  • If there is fuel leakage, inspect the fuel hoses, hose clamps, and fuel pipe sealing surface and replace as necessary.

4. After repair, assemble the system and repeat Steps 1 to 3.