#
CYLINDER BLOCK INSPECTION

B3E011010300201

1.• Measure the distortion of the cylinder block top surface in six directions as indicated in the figure.

  • If it exceeds the maximum, replace the cylinder block.

Maximum cylinder block distortion

  0.10 mm {0.004 in}

2. Measure the cylinder bores in X and Y directions at 42 mm {1.65 in} below the top surface.

  • If not within the specification, replace the cylinder block.

Standard diameter limit

  L8: 83.000-83.030 mm {3.2677-3.2689 in}
  LF, L3, L3 (with variable valve timing mechanism): 87.500-87.530 mm {3.4449-3.4460 in}

Minimum / maximum bore diameter limit

  L8: 82.940-83.090 mm {3.2653-3.2712 in}
  LF, L3, L3 (with variable valve timing mechanism): 87.440-87.590 mm {3.4425-3.4484 in}