#
HOLD INDICATOR LIGHT INSPECTION [FN4A-EL]

BME051721101201

## Inspection of Operation

1. Turn the ignition switch from the LOCK to ON position.

  Note

  • The HOLD indicator light will illuminate if a malfunction exists in any of the EC-AT system components.

2. Verify that the HOLD indicator light is not illuminated.

3. Press the switch and verify that the HOLD indicator illuminates.

  • If the HOLD switch function is not as specified, after inspecting the HOLD switch (See HOLD SWITCH INSPECTION [FN4A-EL].), inspect the terminal voltage of the HOLD indicator light.

## Inspection of Voltage

1. Turn the ignition switch to the ON position.

2. Measure the voltage between terminal 3J and ground.

Voltage | Action
--- | ---
B+ | Go to next step
Other | • Replace METER fuse • Repair wiring harness (METER fuse-instrument cluster)

## Inspection of Continuity

1. Disconnect the instrument cluster connector.

2. Disconnect the TCM connector.

3. Inspect for continuity between instrument cluster connector terminal 1H and PCM terminal 3R.

  • If not as specified, inspect the wiring harness (instrument cluster-PCM).
  • If as specified, go to the next step.

Terminals | Continuity
--- | ---
1H- (PCM 3R) | Yes

4. Inspect for continuity between terminals 1H and 3J.

  • If not as specified, replace the instrument cluster or bulb.

Terminals | Continuity
--- | ---
1H-3J | Yes