#
DTC P0016 [MZR-CD (RF Turbo)]

BME010200001W05

DTC P0016 | Crankshaft position-camshaft position correlation malfunction
--- | ---
DETECTION CONDITION | • PCM monitors input signals from CKP sensor and CMP sensor while engine is running. If input signals from CKP sensor and CMP sensor are misaligned, PCM determines crankshaft position-camshaft position correlation malfunction.
POSSIBLE CAUSE | • CKP sensor malfunction • CMP sensor malfunction • Timing belt is loose • PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY RELATED REPAIR INFORMATION AVAILABILITY • Check for related Service Information availability. • Is any related repair information available? | Yes | Perform repair or diagnosis according to available Service Information. • If vehicle is not repaired, go to next step.
No | Go to next step.
2 | VERIFY DTC P0016 DETECTED AGAIN • Clear DTC from PCM memory using WDS or equivalent. • Start engine. • Is same DTC present? | Yes | Go to next step.
No | Intermittent concern exists. Go to "Intermittent Concern Troubleshooting". (See INTERMITTENT CONCERN TROUBLESHOOTING [MZR-CD (RF Turbo)].)
3 | FOLLOW OTHER DETECTED DTC FIRST • Turn engine switch to OFF. • Start engine. • Have P0336, P0337, P0341, P0342 been detected? | Yes | Go to applicable DTC inspection. (See DTC TABLE [MZR-CD (RF Turbo)].)
No | Go to next step.
4 | INSPECT CKP SENSOR • Inspect CKP sensor. (See CRANKSHAFT POSITION (CKP) SENSOR INSPECTION [MZR-CD (RF Turbo)].) • Is there any malfunction? | Yes | Replace CKP sensor, go to Step 7. (See CRANKSHAFT POSITION (CKP) SENSOR REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)
No | Go to next step.
5 | INSPECT CMP SENSOR • Inspect CMP sensor. (See CAMSHAFT POSITION (CMP) SENSOR INSPECTION [MZR-CD (RF Turbo)].) • Is there any malfunction? | Yes | Replace CMP sensor, go to Step 7. (See CAMSHAFT POSITION (CMP) SENSOR REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)
No | Go to next step.
6 | INSPECT TIMING BELT • Inspect timing belt installation. • Is there any malfunction? | Yes | Reinstall timing belt, go to next step.
No | Go to next step.
7 | VERIFY TROUBLESHOOTING OF DTC P0016 COMPLETED • Make sure to reconnect all disconnected connectors. • Clear DTC from PCM memory using WDS or equivalent. • Start engine. • Is same DTC present? | Yes | Replace PCM, go to next step. (See PCM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)
No | Go to next step.
8 | VERIFY AFTER REPAIR PROCEDURE • Perform "After Repair Procedure". (See AFTER REPAIR PROCEDURE [MZR-CD (RF Turbo)].) • Is there any DTC present? | Yes | Go to applicable DTC inspection. (See DTC TABLE [MZR-CD (RF Turbo)].)
No | Troubleshooting completed.