#
PISTON CONSTRUCTION [AJ]

BME011011010T04

## Construction

• High-heat strengthened aluminum alloy has been adopted on the pistons for excellent thermal conductivity.
• The piston skirt is coated with molybdenum to improve durability.
• Offset pistons have been adopted to reduce piston slapping noise.
• Front mark has been adopted on the upper surface of the piston to prevent mis-assembly of the front/back.
• A full-floating type connection has been adopted on the the piston and connecting rod connection.

1 | Offset
2 | Piston pin center
3 | Cylinder bore center