#
REAR WASHER HOSE REMOVAL/INSTALLATION

BME091967470201

1. Disconnect the negative battery cable.

2. Remove the headliner.

3. Remove the rear washer hose from the clips.

4. Remove the door lock timer unit. (See DOOR LOCK TIMER UNIT REMOVAL/INSTALLATION.)

5. Remove the bolts mounting the PCM.

6. Remove the bolts mounting the blower unit.

7. Move the blower unit to the cooling unit side.

8. Remove the grommet of the rear washer hose.

9. Partially peel off the right side mud guard and remove the rear washer hose from the clip.

10. Remove the rear washer hose from the washer tank.

11. Install in the reverse order of removal.