#
B-PILLAR LOWER TRIM REMOVAL/INSTALLATION

BME091768220201

  Warning

  • Handling the side air bag sensor improperly can accidentally deploy the side air bag module, which may seriously injure you. Read AIR BAG SYSTEM SERVICE WARNINGS before working around the B-pillar areas. (SeeSERVICE WARNINGS.)

  Note

  • The side air bag sensor is located in the B-pillar.

1. Remove the front scuff plate.

2. Remove the rear scuff plate.

3. Remove the power sliding door rear switch. (with power sliding door system)

4. Turn the seaming welt over.

5. Remove the fastener.

6. Disengage clips A using a fastener remover, and remove the B-pillar lower trim.

7. Install in the reverse order of removal.