#
DTC P0336 [MZR-CD (RF Turbo)]

BME010200300W08

DTC P0336 | CKP sensor circuit performance problem
--- | ---
DETECTION CONDITION | • PCM monitors input signal from CKP sensor while engine is running. If input signal from CKP sensor is not proper pulse number, PCM determines CKP sensor circuit performance problem.
POSSIBLE CAUSE | • CKP sensor malfunction • Connector or terminal malfunction • PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY RELATED REPAIR INFORMATION AVAILABILITY • Check for related Service Information availability. • Is any related repair information available? | Yes | Perform repair or diagnosis according to available Service Information. • If vehicle is not repaired, go to next step.
No | Go to next step.
2 | VERIFY DTC P0336 DETECTED AGAIN • Clear DTC from PCM memory using WDS or equivalent. • Start engine. • Is same DTC present? | Yes | Go to next step.
No | Intermittent concern exists. Go to "Intermittent Concern Troubleshooting". (See INTERMITTENT CONCERN TROUBLESHOOTING [MZR-CD (RF Turbo)].)
3 | INSPECT POOR CONNECTION OF CKP SENSOR CONNECTOR • Turn engine switch to OFF. • Inspect for poor connection (damaged, pulled-out terminals, corrosion, etc.). • Is there any malfunction? | Yes | Repair or replace suspected terminal, go to Step 6.
No | Go to next step.
4 | INSPECT CKP SENSOR • Inspect CKP sensor. (See CRANKSHAFT POSITION (CKP) SENSOR INSPECTION [MZR-CD (RF Turbo)].) • Is there any malfunction? | Yes | Replace CKP sensor, go to Step 6. (See CRANKSHAFT POSITION (CKP) SENSOR REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)
No | Go to next step.
5 | INSPECT POOR CONNECTION OF PCM CONNECTOR • Turn engine switch to OFF. • Inspect for poor connection (damaged, pulled-out terminals, corrosion, etc.). • Is there any malfunction? | Yes | Repair or replace suspected terminal, go to next step.
No | Go to next step.
6 | VERIFY TROUBLESHOOTING OF DTC P0336 COMPLETED • Make sure to reconnect all disconnected connectors. • Clear DTC from PCM memory using WDS or equivalent. • Start engine. • Is same DTC present? | Yes | Replace PCM, go to next step. (See PCM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)
No | Go to next step.
7 | VERIFY AFTER REPAIR PROCEDURE • Perform "After Repair Procedure". (See AFTER REPAIR PROCEDURE [MZR-CD (RF Turbo)].) • Is there any DTC present? | Yes | Go to applicable DTC inspection. (See DTC TABLE [MZR-CD (RF Turbo)].)
No | Troubleshooting completed.