#
DIAGNOSTIC MONITORING TEST RESULTS [L3]

BME010200102222

• The purpose of this test mode is to confirm the result of the OBD monitor diagnostic test results. The result values stored when a particular monitored item is completed are displayed. If the monitored item is not completed, initial value is displayed.

TEST ID | Description | Related system
--- | --- | ---
10: 01: 0A | Rich to lean sensor threshold voltage | HO2S
10: 02: 0A | Lean to rich sensor threshold voltage
10: 03: 0A | Low sensor voltage for switching time calculation
10: 04: 0A | High sensor voltage for switching time calculation
10: 05: 10 | Rich to lean sensor switching time
10: 06: 10 | Lean to rich sensor switching time
10: 0A: 10 | Sensor period
10: 80: 20 | Front and Rear HO2S switching time ratio | TWC