#
MANUAL TRANSAXLE SPECIFICATIONS [A65M-R]

BME050000000T06

Item | Specifications
--- | ---
Transaxle type | A65M-R
Engine type | MZR-CD (RF Turbo)
Transaxle control | Floor-shift
Operation system | Cable
Shift assist | Forward | Synchromesh
Reverse
Gear ratio | 1st | 3.416
2nd | 1.789
3rd | 1.193
4th | 0.902
5th | 0.659
Reverse | 3.252
Final gear ratio | 4.133
Oil | Grade | API service GL-4 or GL-5
Viscosity | All season | SAE 75W-90
Capacity (approximate quantity) (L {US qt, Imp qt}) | 2.30 {2.4, 2.0}