#
REAR POWER WINDOW REGULATOR DISASSEMBLY/ASSEMBLY

BME091272560W02

1. Disassemble in the order indicated in the table.

2. Assemble in the reverse order of disassembly.

1 | Cover (See Cover Assembly Note.)
2 | Power window motor (See Power Window Motor Assembly Note.)
3 | Frame (See Frame Assembly Note.)

## Frame Assembly Note

1. Install wire A in part B on the upper of the drum.

## Power Window Motor Assembly Note

  Note

  • The cable must be held to install the drum; install with another person.

1. Press the cable as shown to remove any slack. (1)

2. Install the drum to the power window motor.

## Cover Assembly Note

1. Use long nose pliers to clamp the cover.