#
HEADLIGHT LEVELING SWITCH REMOVAL/INSTALLATION

BME091851030W05

1. Disconnect the negative battery cable.

2. Remove the driver-side side panel.

3. Remove in the order indicated in the table.

4. Install in the reverse order of removal.

1 | Headlight leveling switch (See Headlight Leveling Switch Removal Note.)
2 | Connector

## Headlight Leveling Switch Removal Note

1. Insert your hand into the hole in the driver-side side panel, squeeze the tabs of the headlight leveling switch and pull it forward to remove it.