#
DTC P0223 [MZR-CD (RF Turbo)]

BME010200102268

DTC P0223 | Accelerator pedal position (APP) sensor No.2 circuit high input
--- | ---
DETECTION CONDITION | • The PCM monitors the input signal from accelerator pedal position sensor No.2. If the voltage from accelerator pedal position sensor No.2 is more than 4.7 V, the PCM determines that there is a malfunction in the accelerator pedal position sensor No.2 circuit. Diagnostic support note
• The MIL illuminates if the PCM detects the above malfunction condition in the first drive cycle.
• FREEZE FRAME DATA is available.
• The DTC is stored in the PCM memory.
POSSIBLE CAUSE | • APP sensor No.2 malfunction • Connector or terminal malfunction • Short to power supply in wiring harness between APP sensor terminal C and PCM terminal 88 • Open circuit in wiring harness between APP sensor terminal D and PCM terminal 91 • PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA HAS BEEN RECORDED • Has FREEZE FRAME DATA been recorded? | Yes | Go to the next step.
No | Record the FREEZE FRAME DATA on the repair order, then go to the next step.
2 | VERIFY RELATED REPAIR INFORMATION AVAILABILITY • Verify related service repair information availability. • Is any related repair information available? | Yes | Perform repair or diagnosis according to the available repair information. • If the vehicle is not repaired, go to the next step.
No | Go to the next step.
3 | VERIFY CURRENT SIGNAL STATUS: IS CONCERN INTERMITTENT OR CONSTANT? • Connect the WDS or equivalent to the DLC-2. • Clear the DTC from the PCM memory using the WDS or equivalent. • Start the engine. • Is the same DTC present? | Yes | Go to the next step.
No | Intermittent concern exists. Perform the "INTERMITTENT CONCERN TROUBLESHOOTING". (See INTERMITTENT CONCERN TROUBLESHOOTING [MZR-CD (RF Turbo)].)
4 | INSPECT APP SENSOR CONNECTOR FOR POOR CONNECTION • Turn the engine switch off. • Disconnect the APP sensor connector. • Inspect for poor connection (such as damaged/pulled-out pins, corrosion). • Is there any malfunction? | Yes | Repair or replace the terminal, then go to Step 9.
No | Go to the next step.
5 | INSPECT APP SENSOR NO.2 SIGNAL CIRCUIT FOR SHORT TO POWER SUPPLY • Turn the engine switch to the ON position (Engine off). • Measure the voltage between APP sensor terminal C (wiring harness-side) and body GND. • Is the voltage more than 4.7 V? | Yes | Repair or replace the wiring harness for a possible short to power supply, then go to Step 9.
No | Go to the next step.
6 | INSPECT APP SENSOR NO.2 • Inspect the APP sensor No.2. (See ACCELERATOR PEDAL POSITION (APP) SENSOR INSPECTION [MZR-CD (RF Turbo)].) • Is there any malfunction? | Yes | Replace the APP sensor, then go to Step 9.
No | Go to the next step.
7 | INSPECT PCM CONNECTOR FOR POOR CONNECTION • Turn the engine switch off. • Disconnect the PCM connector. • Inspect for poor connection (such as damaged/pulled-out pins, corrosion). • Is there any malfunction? | Yes | Repair or replace the terminal, then go to Step 9.
No | Go to the next step.
8 | INSPECT APP SENSOR NO.2 GND CIRCUIT FOR OPEN CIRCUIT • Turn the engine switch off. • Inspect for continuity between APP sensor terminal D (wiring harness-side) and PCM terminal 91 (wiring harness-side). • Is there continuity? | Yes | Go to the next step.
No | Repair or replace the wiring harness for a possible open circuit, then go to the next step.
9 | VERIFY TROUBLESHOOTING OF DTC P0223 COMPLETED • Make sure to reconnect all disconnected connectors. • Clear the DTC from the PCM memory using the WDS or equivalent. • Start the engine. • Is the same DTC present? | Yes | Replace the PCM, then go to the next step.
No | Go to the next step.
10 | VERIFY AFTER REPAIR PROCEDURE • Perform the Repair Verification Drive Mode. (See OBD DRIVE MODE [MZR-CD (RF Turbo)].) • Are any DTCs present? | Yes | Go to the applicable DTC inspection. (See DTC TABLE [MZR-CD (RF Turbo)].)
No | DTC troubleshooting completed.