#
MAP LIGHT REMOVAL/INSTALLATION

BME091851310201

## With Sliding Sunroof

1. Disconnect the negative battery cable.

2. Remove in the order indicated in the table.

3. Install in the reverse order of removal.

1 | Map light (See Map light removal note.)
2 | Connector
3 | Lens (See Lens removal note.)
4 | Map light bulb

### Map light removal note

1. Insert a tape-wrapped flathead screwdriver into the gap between the headliner and the map light.

2. Twist the flathead screwdriver.

### Lens removal note

1. Push the tabs of the lens using a tape-wrapped flathead screwdriver, and remove the lens.

## Without Sliding Sunroof

1. Disconnect the negative battery cable.

2. Remove in the order indicated in the table.

3. Install in the reverse order of removal.

1 | Screw
2 | Overhead console
3 | Connector
4 | Lens (See Lens removal note.)
5 | Map light bulb
6 | Holder

1 | Map light (See Map light removal note.)
2 | Connector
3 | Lens (See Lens removal note.)
4 | Map light bulb

### Lens removal note

1. Push the tabs of the lens using a tape-wrapped flathead screwdriver, and remove the lens.