#
VEHICLE SPEED SENSOR (VSS) INSPECTION [JA5A-EL]

BME051717400201

## On-Vehicle Inspection

1. Disconnect the terminal component No.2 connector.

2. Measure resistance between the terminals A and B.

  • If not within the specification, inspect the VSS. (See Individual Part Inspection.)

Resistance (ATF temperature: 20 °C {68 °F})

  513-627 ohms

3. Connect the terminal component No.2 connector.

## Individual Part Inspection

1. Remove the VSS. (See VEHICLE SPEED SENSOR (VSS) REMOVAL/INSTALLATION [JA5A-EL].)

2. Measure resistance between the terminals of the VSS.

  • If not within the specification, replace the VSS.
  • If it is normal, replace the harness.

Resistance (ATF temperature: 20 °C {68 °F})

  513-627 ohms

3. Install the VSS. (See VEHICLE SPEED SENSOR (VSS) REMOVAL/INSTALLATION [JA5A-EL].)