#
NO.5 NO CREEP AT ALL [FN4A-EL]

BME050301030209

5 | No creep at all
DESCRIPTION | • Either the transaxle is stuck in 3GR position, or there is clutch circuit slippage
POSSIBLE CAUSE | • Either transaxle is stuck in 3GR or 4GR position, or there is clutch circuit slippage due to a stuck 3-4 clutch.

  1. Clutch burnt

  • Line pressure low
  • Shift solenoid D malfunction
  • Shift solenoid A malfunction
  • Shift solenoid B malfunction
  • Shift solenoid C malfunction
  • Pressure control solenoid malfunction
  • Body GND malfunction
  • Control valve body malfunction

  2. Transaxle fixed in 3GR (Operation of fail-safe function)

  • Short or open circuit in wiring harness
  • Poor connection of connector
  • Malfunction of electronic parts of output and input system

  3. There is no engine torque

  • Torque converter malfunction

  Note

  • Before following the troubleshooting steps, make sure that the Automatic Transaxle On-Board Diagnostic and Automatic Transaxle Basic Inspection are conducted.

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | Does the vehicle creep in any range/position? | Yes | Go to the next step.
No | Inspect or adjust the selector lever. (See SELECTOR LEVER REMOVAL/INSTALLATION.)
2 | Inspect the value at the following PCM PID using the WDS or equivalent. (See PCM INSPECTION [L3].) • TP Is the PID value normal? | Yes | Go to the next step.
No | Repair or replace any malfunctioning parts.
3 | Disconnect the PCM connector. Is the resistance between the ground terminal at the PCM connector and body the ground less than 5.0 ohms? | Yes | Go to the next step.
No | Repair open ground circuit.
4 | Inspect the LPS PID value using the WDS or equivalent. Is the LPS PID value normal? (See PCM INSPECTION [L3].) | Yes | Overhaul the control valve body and repair or replace any malfunctioning parts. (See ATX workshop manual (FN4A-EL).) If any problem remains, overhaul the transaxle and repair or replace any malfunctioning parts. (See ATX workshop manual (FN4A-EL).)
No | Repair or replace any malfunctioning parts.